UAT geneos gateway install

1) cd /usr/local/itrs.

2) /etc/init.d/itrs\_gateway stop

3) cp –pr  gateway2.linux.GA3.0.23-141114  gateway2.linux.GA3.0.23-141114.preupgrade.

4) mv gateway2.linux.GA3.0.23-141114  gateway2.linux\_64.GA3.1.2-150714

5) cp gateway2.linux\_.GA3.1.2-150714.tar.gz  ./gateway2.linux\_64.GA3.1.2-150714

6) cd gateway2.linux\_.GA3.1.2-150714;

7) tar –zxvf gateway2.linux\_.GA3.1.2-150714.tar.gz

8) chown –Rh netagent: netagent \*

8) cd ..

9a) rm gateway.uat

9) ln –s gateway2.linux\_64.GA3.1.2-150714 gateway.uat

10) /etc/init.d/itrs\_gateway.dev start

There may be a couple of addional steps

Tony, off the back of this and to enable me to test the netprobe deployment, could you also copy the following files to the UAT gateway as follows;

[\\ldnfs4\ebrepository\geneos\GA3.1.2\netprobe.windows.GA3.1.2-150722.zip](file://ldnfs4/ebrepository/geneos/GA3.1.2/netprobe.windows.GA3.1.2-150722.zip)

[\\ldnfs4\ebrepository\geneos\GA3.1.2\netprobe.linux\_64.GA3.1.2-150722.tar.gz](file://ldnfs4/ebrepository/geneos/GA3.1.2/netprobe.linux_64.GA3.1.2-150722.tar.gz)

Copy both files (un-extracted) to /usr/local/itrs/gateway.uat